What should I plan to skip in the CCIE lab?

VLOG:

skip dampening?

lab tracker update

6 bgp labs left then mpls

MEAT CHUNKS:

WHIP-CRACKING:

- bgp fast failover

- bgp outbound route filtering

command combos:

sh run int x/x / sh run | sec {technology / ping / tracert

sh run | sec router ospf

conf t

logging buffered debug

logging buffer 1000000

end

clear log