A cruel OSPF PE CE lab

:: VLOG TOPICS ::

OSPF PE-CE routing

MPLS Configuration on Cisco IOS Software

Lab router preconfigs?

line con 0

exec-timeout 0 0

logging synchronous

line vty 0 15

exec-timeout 0 0

logging synchronous

no ip domain-lookup

:: MEAT CHUNKS (links OTD) ::

Kevin Wallace’s CCIE time saver tips:

<https://www.youtube.com/watch?v=C9EQDZRD-vg&t=0s>

Catalyst vs NX-OS trunks:

<https://www.netcraftsmen.com/troubleshooting-trunks-in-a-nx-os-environment-to-trunk-or-not-to-trunk/>

RFC 4577 OSPF PE-CE

<https://tools.ietf.org/html/rfc4577>

::WHIP CRACKING (labs)::

PE-CE Routing with OSPF

:: SOCIAL MEDIA ::

DISCORD - https://discord.gg/wHPTNa

TWITTER - https://twitter.com/thelantamer

INSTAGRAM - https://www.instagram.com/thelantamer/

FACEBOOK - https://www.facebook.com/lantamer/

:: LAB LINKS ::

Google docs share - http://bit.ly/2AbJQhp

INE Diagrams - http://bit.ly/2mgTGso

INE VIRL files on Github - http://bit.ly/2ht78YH