VLOG:

bgp remove private-as, dampening labs

MEAT CHUNKS:

In defense of NATs:

http://www.circleid.com/posts/20170905\_an\_opinion\_in\_defence\_of\_nats/

Battlefield tactics part 1:

https://learningnetwork.cisco.com/blogs/unleashing-ccie-rs/2014/11/07/battlefield-tactics-part-1

Battlefield tactics part 2:

https://learningnetwork.cisco.com/blogs/unleashing-ccie-rs/2014/12/08/battlefield-tactics-part-2

WHIP-CRACKING:

- bgp remove private as

- dampening

- dampening with route-map

command combos:

sh run int x/x / sh run | sec {technology / ping / tracert

sh run | sec router ospf

sh run | s access-list

sh run | s prefix-list

conf t

logging buffered debug

logging buffer 1000000

end

clear log